Hood Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Hood Hold-Open Device Caution in the Preface section.

Important: Install the protective coverings over the fenders and the windshield in order to prevent damage to the paint, the glass, and the moldings when you are removing and installing the hood.

1. Raise and support the hood.
2. Remove the hood bolts (1).
3. Remove the hood (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the hood with the bolts.

Tighten
Tighten the hood hinge to hood bolts to 25 N·m (18 lb ft).

2. Inspect the hood for proper alignment.