Noise in Steering Column. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---

Improperly installed intermediate shaft-to-column joints

• | Tighten the coupling pinch bolts.

• | Replace the intermediate shaft as needed.

Column misalignment | Replace the alignment spacer.
The lack of lubrication for the joint | Lubricate the joint.
The lack of lubrication for the steering shaft | Lubricate the steering shaft bearing.

Improperly seated shaft lock snap ring

• | Adjust the shaft lock snap ring.

• | Replace the shaft lock snap ring as needed.

Improperly installed intermediate shaft pinch bolt | Tighten the pinch bolt.