Transmission Control Module Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the connectors.
3. Remove the transaxle control mode (TCM) mounting bolts and TCM.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the TCM mounting bolts and TCM.

Tighten
Tighten the mounting bolts to 6 N·m (53 lb in).

2. Connect the connectors.
3. Connect the negative battery cable.