Rear Window Washer Nozzle Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the rear spoiler from the tailgate. Refer to Liftgate Trim Panel Replacement .
2. Remove the center high mounted stop lamp (CHMSL) from the tailgate. Refer to High Mount Stop Lamp Replacement .
3. Remove the washer hose from the nozzle.
4. Remove the washer nozzle.

### Installation Procedure

1. Install the nozzle on the tailgate.
2. Connect the washer hose to the nozzle.
3. Install the CHMSL to the tailgate. Refer to High Mount Stop Lamp Replacement .
4. Install the rear spoiler. Refer to Liftgate Trim Panel Replacement .