Rear Seat Back Cushion Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back lock by pulling the lock knob upward (1).
2. Remove the seat back hinge bolts (2).
3. Remove the rear seat back (3).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat back with the hinge bolts (1).

Tighten
Tighten the hinge bolts to 23-28 N·m (17-21 lb ft).

2. Press the lock knob.