Power Steering Pump Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Important: The power steering pump in this vehicle is not serviceable. A faulty pump must be replaced.

1. Remove the front passenger side headlamp.
2. Disconnect the supply line pipe hose (1).
3. Disconnect the pressure line pipe fitting (2).
4. Remove the pump drive belt. Refer to Power Steering Pump Belt Replacement .

5. Disconnect the power steering pressure switch connector (1) and remove the bolts (2).
6. Remove the power steering pump and bolt (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the power steering pump with the bolt (1).

Tighten
Tighten the bolt to 18-22 N·m (13-16 lb ft).

2. Connect the power steering pressure switch connector.
3. Install the pump drive belt. Refer to Power Steering Pump Belt Replacement .
4. Install the rear bracket adjusting (2) and power steering bolt (3).

Tighten

• | Tighten the rear bracket adjusting bolt to 20-24 N·m (15-18 lb ft).

• | Tighten the power steering bolt to 20-24 N·m (15-18 lb ft).

5. Connect the pressure line pipe to the outlet connection (1) on the steering pump.

Tighten
Tighten the pressure line pipe fitting to 21-35 N·m (16-26 lb ft).

6. Install the front passenger side headlamp.
7. Refill the pump with new fluid and bleed the air from the system. Refer to Power Steering System Bleeding .
8. Inspect for leaks. If leaks are found, correct the cause of the leak and bleed the system.