Driver or Passenger Seat Belt Buckle Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front seat belt buckle bolt (3).

Important: Before removing the driver seat belt buckle, disconnect the reminder light connector.

2. Remove the front seat belt buckle (1).
3. Remove the front seat belt buckle patch (2).

### Installation Procedure

Caution: Refer to Seat Belt Replacement Caution in the Preface section.

1. Connect the reminder light connector.
2. Install the front seat belt buckle patch.
3. Install the front seat belt buckle.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the front seat belt buckle bolt (1).

Tighten
Tighten the seat belt buckle bolt to 30-45 N·m (22-33 lb ft).