Rear Wheel Speed Sensor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the rear wheel speed sensor electrical connector (1).
3. Remove the rear wheel speed sensor bolt (2).
4. Remove the rear wheel speed sensor (1) from the backing plate.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear wheel speed sensor (1) to the backing plate. Secure it with the bolt (2).

Tighten
Tighten the rear wheel speed sensor bolt to 11 N·m (97 lb in).

2. Connect the rear wheel speed sensor electrical connector (1).
3. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .