Blower Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the control assembly. Refer to Heater and Air Conditioning Control Replacement .
2. Remove the switch knob (1).
3. Remove the blower motor switch retaining screw (1).
4. Turn the blower motor switch counterclockwise (2).
5. Remove the blower motor switch.

### Installation Procedure

1. Install the blower motor switch with the screw.
2. Install the switch knob.
3. Install the control assembly. Refer to Heater and Air Conditioning Control Replacement .