Liftgate Window Strut Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Open the tailgate and suitably support it.
2. Remove the rear body end fitting nut from the ball studs (2).
3. Remove the tailgate end fitting nut from the ball studs (1).
4. Remove the tailgate strut assembly.

### Installation Procedure

1. Install the tailgate end fitting nut to the ball studs.
2. Install the rear body end fitting nut to the ball studs.
3. Install the tailgate strut assembly.