Clutch Cable Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the clutch cable adjusting nut.
2. Disconnect the clutch cable from the wire clip.
3. Pull and remove the clutch cable from the transaxle mount hole.
4. Disconnect the clutch cable from the pedal by pulling upward and disconnecting the cable from the pedal hook (1).
5. Remove the battery. Refer to Battery Replacement .
6. Remove the clutch cable nuts (2).
7. Remove the cable grommet (1).
8. Remove the clutch cable from the pedal (3).

### Installation Procedure

1. Install the clutch cable.
2. Install the battery. Refer to Battery Replacement .

Caution: Refer to Batteries Produce Explosive Gases Caution in the Preface section.

3. Connect the clutch cable to the pedal.
4. Connect the clutch cable to the transaxle.
5. Adjust the clutch cable. Refer to Clutch Assembly Adjustment .