Quarter Window Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the front door seal trim. Refer to Door Water Deflector Replacement .
2. Remove the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
3. Remove the guide rail screw (1).
4. Remove the inside bolt (2).
5. Remove the outside bolt (3).
6. Remove the division bar (4).
7. Remove the guide rail.
8. Remove the quarter glass assembly (1) from the front door.
9. Remove the quarter glass run (2).

### Installation Procedure

1. Install the quarter glass with the quarter glass run.
2. Install the division bar with the guide rail inside bolt, the guide rail outside bolt and the guide rail screw.
3. Inside the outside rearview mirror. Refer to Outside Rearview Mirror Replacement .
4. Install the front door seal trim. Refer to Door Water Deflector Replacement .