Instrument Cluster Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster trim panel from the instrument panel. Refer to Instrument Panel Outer Trim Cover Replacement .
3. Remove the instrument cluster assembly screws (2).
4. Disconnect the electrical connector.
5. Remove the instrument cluster assembly (1) from the instrument panel.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Connect the electrical connector.
2. Install the instrument cluster assembly (1) to the instrument panel with the screws (2).

Tighten
Tighten the screws to 4 N·m (35 in lb).

3. Install the instrument cluster trim panel to the instrument panel. Refer to Instrument Panel Outer Trim Cover Replacement .
4. Connect the negative battery cable.