Front Side Door Outside Handle Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the front door lock rods.
3. Remove the outside front door handle bolts (2).
4. Remove the outside front door handle (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outside front door lock handle (1) with the bolts (2).

Tighten
Tighten the bolts to 4.5 N·m (40 in lb).

2. Install the front door lock rods.
3. Connect the negative battery cable.