Radio Front Speaker Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door water deflector. Refer to Door Water Deflector Replacement .
3. Remove the speaker screws (2).
4. Disconnect the speaker electrical connector.
5. Remove the speaker (1).

### Installation Procedure

1. Connect the electrical connector.
2. Install the speaker with the screws.
3. Install the door water deflector. Refer to Door Water Deflector Replacement .
4. Connect the negative battery cable.