Windshield Wiper and Washer Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the steering column cover. Refer to Steering Column Trim Covers Replacement .
3. Remove the wiper switch.

3.1. | Disconnect the wiper switch by pushing the locking from the switch housing (1).

3.2. | Disconnect the connector (2).

### Installation Procedure

1. Install the wiper switch.
2. Install the steering column cover. Refer to Steering Column Trim Covers Replacement .
3. Connect the negative battery cable.