Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Nuts | 9-12 N·m | 80-106 lb in
Battery Carrier Tray Bolts | 9-12 N·m | 80-106 lb in
Battery Retainer Clamp-to-Battery Rod Nuts | 6-8 N·m | 53-71 lb in
Distributor Bolts | 10-16 N·m | 89-142 lb in
Generator Battery Lead Connector Nut | 4-7 N·m | 35-62 lb in
Generator Bearing Plate Bolt | 6-8 N·m | 53-71 lb in
Generator Belt Tension Adjusting Bolt | 18-28 N·m | 13-21 lb ft
Generator Brush Holder/Rectifier Screw | 9-12 N·m | 80-106 lb in
Generator Drive End Nut | 80-110 N·m | 59-81 lb ft
Generator Lower Bracket-to-Generator Bolt/Nut | 18-28 N·m | 13-21 lb ft
Generator Shackle Bracket Bolt | 45-55 N·m | 33-41 lb ft
Generator Through-Bolts | 4-6 N·m | 35-53 lb in
Ground Bolt | 35-41 N·m | 26-30 lb ft
Ignition Coil Bracket Bolt | 9-12 N·m | 80-106 lb in
Ignition Coil Screw | 4-7 N·m | 35-62 lb in
Spark Plug | 20-30 N·m | 15-22 lb ft
Starter Field Connector Nut | 9-12 N·m | 80-106 lb in
Starter Mounting Bolts | 55-65 N·m | 41-48 lb ft
Starter Solenoid Assembly Screws | 6-8 N·m | 53-71 lb in
Starter Solenoid Nuts | 9-12 N·m | 80-106 lb in
Starter Through-Bolts | 4-6 N·m | 35-53 lb in