Power Steering Fluid Reservoir Outlet Hose Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the supply line hose from the inlet connection on the power steering pump and drain the power steering fluid (1).
2. Catch the escaping fluid in a drain pan.
3. Disconnect the supply line hose from the power steering fluid reservoir (1).
4. Plug the openings in the power steering pump and the fluid reservoir to prevent fluid loss and contamination.

### Installation Procedure

1. Connect the supply line hose to the power steering fluid reservoir.
2. Connect the supply line hose to the inlet connection on the power steering pump.
3. Fill the fluid reservoir with power steering fluid.
4. Inspect for leaks. If there are leaks, correct the cause of the leaks and bleed the system. Refer to Power Steering System Bleeding .