Windshield Washer Nozzle Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
2. Remove the washer nozzle hose (2).
3. Remove the washer nozzle (1) from the air inlet grille.

### Installation Procedure

1. Install the washer nozzle to the air inlet grille.
2. Install the washer nozzle hose to the washer nozzle.
3. Install the air inlet grille. Refer to Air Inlet Grille Panel Replacement .