Front Side Door Lock Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable, if equipped with the central door lock system.
2. Remove the seal trim. Refer to Door Water Deflector Replacement .
3. Disconnect the outside door handle rod (1) from the door lock.
4. Remove the front door lock screws (2).
5. Remove the front door lock (1).
6. Disconnect the actuator connector, if equipped with the central door lock system.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front door lock (1) with screws (2).

Tighten
Tighten the screws to 8 N·m (71 in lb).

2. Connect the actuator connector, if equipped with the central door lock system.
3. Connect the outside door handle rod (1) and the key rod to the door lock.
4. Install the seal trim. Refer to Door Water Deflector Replacement .
5. Connect the negative battery cable, if equipped with the central door lock system.