Brake Assist System Diagnosis. Chevrolet Joy 2008

For 1990-2009 cars

1. With the engine stopped, eliminate the vacuum in the booster by pumping the brake pedal several times.
2. Push the pedal down and hold it in this position.
3. Start the engine.
4. The booster is OK if the pedal drops further because of extra force produced.

If the brake pedal does not drop, the vacuum system, such as vacuum hoses, check valve, etc. are probably defective and should be checked. If no defect is revealed by checking the vacuum system, the defect is in the booster itself.

### Check Valve Functional Check

1. Remove the vacuum hose.
2. Suck the vacuum hose to power booster. And also, suck the vacuum hose to engine.
3. If the air pass through the check valve or not, replace the check valve. And if the vacuum hose to engine is only sucked, the check valve OK.