Stop Lamp Switch Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the connector (1), LHD shown, RHD similar.
3. Turn the stop lamp switch (2), LHD shown, RHD similar.
4. Remove the stop lamp switch, LHD shown, RHD similar.

### Installation Procedure

Important: After installing the stop lamp switch, pull the lever completely.

1. Install the stop lamp switch, LHD shown, RHD similar.
2. Connect the electrical connector.
3. Connect the negative battery cable.