Exhaust Manifold Installation. Chevrolet Joy 2008

For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the exhaust manifold to the pup-up catalytic converter bolts.

Tighten
Tighten the exhaust manifold to the pup-up catalytic converter bolts to 50-60 N·m (36-43 lb ft).

2. Install the exhaust manifold with pup-up catalytic converter.

Tighten
Tighten the exhaust manifold bolts and nuts to 17-27 N·m (13-20 lb ft).

3. Install the exhaust pipe to the pup-up catalytic converter.

Tighten
Tighten the exhaust pipe to the pup-up catalytic converter nuts to 25-35 N·m (18-25 lb ft).

4. Install the exhaust manifold heat shield.

Tighten
Tighten the exhaust manifold heat shield bolts to 8-12 N·m (71-106 lb in).

5. Connect the O2S sensor connector and ignition wire.
6. Install snorkel assembly, resonator and filter. Refer to Air Cleaner Assembly Replacement .