Windshield Washer Solvent Container Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the washer reservoir inlet bolt.
3. Remove the washer reservoir inlet.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

4. Raise and suitable support the vehicle. Refer to Lifting and Jacking the Vehicle .
5. Remove the front RH wheelhouse splash shield screws.
6. Remove the front RH wheelhouse splash shield clips.
7. Remove the front RH wheelhouse splash shield.

### Installation Procedure

1. Install the washer reservoir assembly with the bolts.
2. Connect the washer pump electrical connector.
3. Connect the washer hose connector.
4. Install the front RH wheelhouse splash shield with the screws and the clips.
5. Lower the vehicle.
6. Install the washer reservoir with the bolt.
7. Connect the negative battery cable.