Rear Door Lock Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable, if equipped with the central door lock system.
2. Remove the door trim panel. Refer to Rear Side Door Trim Panel Insert Replacement .

Important: In case of the deluxe type, remove the seal trim after removing the door pocket handle bracket.

3. Remove the water deflector (1). Refer to Door Water Deflector Replacement .
4. Remove the door pocket handle bracket (2).
5. Remove the screw (2).
6. Remove the guide piece (1).
7. Disconnect the outside door handle rod (1) from the door lock.
8. Disconnect the actuator connector, if equipped with the central door lock system.
9. Remove the door lock screws (2).
10. Remove the door lock (1) from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear door lock (1) with the screws (2).

Tighten
Tighten the screws to 8 N·m (71 in lb).

2. Connect the actuator connector, if equipped with the central door lock system.
3. Connect the outside door handle rod (1) to the door lock.
4. Install the guide rail (1) with the screw.

Tighten
Tighten the screw to 7 N·m (62 in lb).

5. Install the water deflector. Refer to Door Water Deflector Replacement .
6. Install the door trim panel. Refer to Rear Side Door Trim Panel Insert Replacement .
7. Connect the negative battery cable, if equipped with the central door lock system.