Parking Brake Lever Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the parking brake lever cover. Refer to Front Floor Console Replacement .
2. Remove the parking brake cable cover screw (1).
3. Remove the parking brake cable cover (2).
4. Disconnect the brake warning lamp switch (1).

Important: Ensure the parking brake lever is in a fixed position.

5. Remove the brake warning switch lamp screw (2).
6. Remove the park brake lever bolts (2) and nut (1).
7. Remove the park brake lever cotter pin and remove the pin.

### Installation Procedure

1. Install the park brake lever.
2. Install the pin.
3. Install the cotter pin.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the parking brake lever nut (1) and bolts (2).

#### Tighten

• | Tighten the parking brake nut to 10 N·m (89 lb in).

• | Tighten the parking brake bolts to 10 N·m (89 lb in).

5. Connect the brake warning lamp switch.
6. Install the brake warning lamp switch screw.
7. Install the parking brake cable cover.
8. Install the parking brake cable cover screw.
9. Install the parking brake lever cover. Refer to Front Floor Console Replacement .