Brake Rotor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the steering knuckle. Refer to Steering Knuckle Replacement .
2. Remove the rotor bolts from the front wheel hub.
3. Remove the rotor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rotor to the front wheel hub by tightening the detent bolts (1).

Tighten
Tighten the rotor-to-front wheel hub detent bolts to 65 N·m (48 lb ft).

2. Install the steering knuckle. Refer to Steering Knuckle Replacement .