Theft Deterrent Module Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the control module/receiver electrical connector.
3. Slide the control module/receiver away from its mounting bracket.

### Installation Procedure

1. Install the control module/receiver on its mounting bracket.
2. Connect the control module/receiver electrical connector.
3. Connect the electrical battery cable. Refer to Battery Negative Cable Disconnection and Connection .
4. Refer to Control Module References for programming and setup information.