Loss of Coolant. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---
A leak in the radiator | Replace a damaged radiator.
A leak in the surge tank or the hose | Replace the surge tank or the hose.

Looseness or damage of radiator hoses, heater hoses, or connections

• | Reseat the hoses.

• | Replace the hoses or the clamps.

Leaks in the coolant pump seal | Replace the coolant pump seal.
Leaks in the coolant pump gasket | Replace the coolant pump gasket.

An improper cylinder head torque

• | Tighten the cylinder head bolts to specifications.

• | Replace the cylinder head gasket, if needed.

Leaks in the intake manifold, cylinder head gasket, heater core | Repair or replace any components, as needed to correct the leak.