Air Cleaner Element Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the air filter element bolts (1).
2. Remove the air filter upper housing with connecting manifold air temperature sensor with intake tube (2).
3. Remove the air filter element (3).

### Installation Procedure

1. Install the air filter element (3).
2. Install the air filter upper housing by connecting the manifold air temperature sensor to the intake tube (2).
3. Install the air filter element bolts.