Exhaust Gas Recirculation Valve Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Caution: Refer to Exhaust Gas Recirculation (EGR) System Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
3. Disconnect the electric exhaust gas recirculation (EGR) valve connector.
4. Remove the EGR valve.

### Installation Procedure

1. Install the EGR valve.
2. Connect the EGR valve connector.
3. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
4. Connect the negative battery cable.