Steering Wheel Kickback. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---
Contaminated air in the power steering system | Bleed the power steering system.
Worn or damaged wheel bearings | Replace the wheel bearings.
Loose steering gear mounting | Tighten the steering gear mounting bracket bolts.
Improperly installed steering gear-to-intermediate shaft joints | Tighten the joint bolt.

Loose tie rods and ball joints

• | Tighten the tie rods and the ball joints.

• | Replace the tie rods and the ball joints as needed.