Windshield Washer Hose Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
3. Disconnect the washer hose connector.
4. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
5. Remove the front wheel. Refer to Tire and Wheel Removal and Installation .
6. Remove the screws and the front wheel well splash shield.
7. Disconnect the washer hose from the washer pump.
8. Remove the washer hose.

### Installation Procedure

1. Install the washer hose.
2. Connect the washer hose to the washer pump.
3. Install the front wheelhouse splash shield with the screws and the clips.
4. Install the front wheel. Refer to Tire and Wheel Removal and Installation .
5. Lower the vehicle.
6. Connect the washer hose connector.
7. Install the air inlet grille. Refer to Air Inlet Grille Panel Replacement .