Discharge Hose Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
3. Remove the discharge pipe line nut.
4. Remove the discharge pressure pipe line.

### Installation Procedure

1. Install the discharge pipe line.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the discharge pipe line nut.

Tightening
Tighten the discharge pipe line nut to 22.5 N·m (16.5 lb ft).

3. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
4. Recharge the A/C refrigerant. Refer to Refrigerant Recovery and Recharging .