Clutch Release Arm Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the clutch cable adjusting nut (1).
2. Disconnect the clutch cable (2).
3. Remove the clutch release arm bolt and nut (2).
4. Remove the clutch release arm (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the clutch release arm matching to punched mark (1).
2. Install the clutch release arm.

Tighten
Tighten the bolt and nut to 10-16 N·m (7.5-12 lb ft).

3. Adjust the clutch cable. Refer to Clutch Assembly Adjustment .