Engine Oil and Oil Filter Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Raise and properly support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Position an appropriate drain pan under the engine.
3. Remove the oil pan drain plug bolt.
4. Remove the oil filter.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil filter.

Tighten
Tighten the oil filter to 12-16 N·m (106-140 lb in).

2. Discard the used oil pan drain plug washer and replace with a new oil pan drain plug washer.
3. Install the oil pan drain plug bolt.

Tighten
Tighten the oil pan drain plug bolt to 30-40 N·m (22-30 lb ft).

4. Lower the vehicle.
5. Fill the engine with oil to the appropriate mark.
6. Start engine and inspect for leaks.