Washer Pump Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the washer reservoir assembly. Refer to Windshield Washer Solvent Container Replacement.
3. Drain the washer fluid.
4. Remove the wiper motor from the washer reservoir assembly.

### Installation Procedure

1. Install the wiper motor to the washer reservoir assembly.
2. Install the washer reservoir assembly. Refer to Windshield Washer Solvent Container Replacement.
3. Connect the negative battery cable.
4. Fill the washer reservoir.