Windshield Wiper Motor Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the windshield wiper arm. Refer to Windshield Wiper Blade Replacement .
3. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
4. Separate the wiper motor from the wiper linkage.
5. Remove the wiper linkage ball from the wiper linkage.
6. Disconnect the electrical connector.
7. Remove the bolts.

Important: Because the wiper motor link plate is fixed, do not separate the wiper motor from the bracket.

8. Remove the wiper motor assembly.
9. Remove the wiper motor from the engine compartment.

### Installation Procedure

1. Install the wiper motor to the engine compartment with the bolts.
2. Connect the electrical connector.
3. Install the wiper linkage to the wiper motor linkage ball.
4. Install the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
5. Install the windshield wiper arm. Refer to Windshield Wiper Blade Replacement .
6. Connect the negative battery cable.