Interior Courtesy Lamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the interior courtesy lamp lens (2).
3. Remove the interior courtesy lamp screws (3).
4. Disconnect the interior courtesy lamp electrical connector (1).
5. Remove the interior courtesy lamp (4).

### Installation Procedure

1. Connect the electrical connector.
2. Install the interior courtesy lamp with the screws.
3. Install the interior courtesy lamp lens.
4. Connect the negative battery cable.