Door Hinge Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the hinge-to-body bolts (3).
2. Remove the hinge-to-door bolts (2).
3. With the aid of another technician, remove the door hinge (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. With the aid of another technician, install the hinge to the door and the body.
2. Install the hinge-to-door bolts (2).
3. Install the hinge-to-body bolts (3).
4. Adjust the door to proper fit.

Tighten

• | Tighten the hinge to body bolts to 35 N·m (26 ft lb).

• | Tighten the hinge to door bolts to 15 N·m (11 ft lb).