Poor Return of Steering Wheel. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Actions
--- | ---
Improperly contacted the steering wheel with the turn signal housing. | Adjust the turn signal housing.
Improper binding or looseness of steering coupling | Replace the intermediate shaft.
Stuck and improperly aligned power steering pump flow control valve | Replace the power steering pump.
Improper binding or looseness of tie rods and ball joints | Tighten the tie rods and the ball joints. Replace the tie rods and the ball joints as needed.
Poor adjustments of the steering gear | Perform a straight-ahead check.