Spark Plug Wire Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Disconnect the spark plug wire at each spark plug.

• | Twist each spark plug boot 1/2 turn before removing.

• | Pull only on the boot or use a tool designed for this purpose in order to remove the wire from each spark plug.

3. Disconnect the spark plug wire from the coil.

• | Twist each spark plug boot 1/2 turn before removing.

• | Pull only on the boot or use a tool designed for this purpose in order to remove the wires from the coil.

### Installation Procedure

1. Install the spark plug wire on the coil.
2. Install the spark plug wire at each spark plug.
3. Inspect the wires for proper installation:

• | Push down on each boot in order to inspect the seating.

• | Reinstall any loose boot.

• | Wire routing must be kept intact during service and followed exactly when wires have been disconnected or when replacement of the wires is necessary. Failure to route the wires correctly can lead to radio interference and crossfire of the plugs, or shorting of the leads to the ground.

• | Any time the spark plug wires or boots are installed on the spark plugs, new dielectric grease needs to be applied inside the boot.