Front Bumper Fascia Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

2. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Remove the front wheels. Refer to Tire and Wheel Removal and Installation.
4. Remove the front fender liner. Refer to Fender Liner Replacement.
5. Remove the bolts (1) on both side of the fascia.
6. Remove the clips (1) under the fascia.
7. Lower the vehicle.
8. Remove the front bumper fascia bolts (1).
9. Remove the clips (1).
10. Remove the front bumper fascia (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the bumper fascia (2).
2. Install the clips on the top of the fascia (1).

Caution: Refer to Vehicle Lifting Caution in the Preface section.

3. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
4. Install the clips (1) under the fascia.
5. Install the bolts (1) on both sides of the fascia.
6. Install the front fender liner. Refer to Fender Liner Replacement.
7. Install the front wheels. Refer to Tire and Wheel Removal and Installation.
8. Lower the vehicle.
9. Connect the negative battery cable.