Starter Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine oil temperature sensor to disconnect the harness connector (2).
3. Remove the starter solenoid nut to disconnect the electrical cable (1).
4. Remove the harness clip bolt to disconnect the harness clip (4).
5. Remove the ground bolt (3).
6. Disconnect the electrical connector and clip around the starter.
7. Remove the starter mounting bolts (2).
8. Remove the starter assembly (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the starter mounting bolts (1).

Tighten
Tighten the bolts to 55-65 N·m (41-48 lb ft).

2. Install the starter solenoid nut (2).

Tighten
Tighten the nut to 9-12 N·m (80-106 lb in).

3. Install the harness clip bolt (2).

Tighten
Tighten the bolt to 9-12 N·m (80-106 lb in).

4. Install and tighten the ground bolt (3).

Tighten
Tighten the bolt to 35-41 N·m (26-30 lb ft).

5. Connect the negative battery cable.