Control Valve Lower Body Assemble. Chevrolet Joy 2008

For 1990-2009 cars

Important:

• | Before assembly, wash all the components thoroughly.

• | Apply AT fluid to all of the components and holes.

• | Do not use components which may have been dropped.

• | With plastic tape, tape the screwdrivers and rods to be used for inserting the valve.

• | Note the orientation of valves and plugs.

1. Install the low clutch accumulator (1).
2. Install the throttle pressure accumulator (4).
3. Install 1-2 accumulator (3).
4. Install the torque converter relief valve (2).