Engine Protection Shield Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Raise and support vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the bolts, then the engine protection shield.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install engine protection shield, and secure with the engine protection shield bolts.

Tighten
Tighten the engine protection shield bolts to 23 N·m (17 lb ft).

2. Lower the vehicle. Refer to Lifting and Jacking the Vehicle .