Front Side Door Trim Panel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

#### Tools Required

J 21104-B (KM 475-B) Trim Remover

### Removal Procedure

1. Remove the door pull screws.
2. Remove the door pull from the front door.
3. Remove the power window switch, if equipped.
4. Remove the inside door handle screw (3).
5. Disconnect the inside door handle rod (1).
6. Pry off the inside door handle (2).
7. Using a cloth, pull out the window regulator handle clip (2).
8. Remove the window regulator handle (1) from the front door.

Important: Make sure to cover the remover with a cloth to prevent paint damage to the door.

9. Pry off the trim panel using a J 21104-B (1) .

### Installation Procedure

1. Install the trim panel.
2. Install the window regulator handle with the clip.
3. Install the power window switch, if removed.
4. Install the inside door handle and the door pull with the screws.