Rear Side Door Sill Trim Plate Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion.
2. Remove the rear seat belt bolt (1) on the floor.
3. Remove the spacer and the spring washer (2).
4. Remove the plastic protector from the seat belt anchor.
5. Remove the screws securing the rear rocker trim panel (2).
6. Remove the rear rocker trim panel clip (3).
7. Pry off the rear rocker trim panel (1).

### Installation Procedure

1. Install the rear rocker trim panel with the screws and the clip.
2. Install the rear seat belt bolt on the floor.
3. Install the rear seat cushion.