Evaporative Emission Canister Vent Solenoid Valve Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Fuel and Evaporative Emission Pipe Caution in the Preface section.

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

Caution: Refer to Safety Goggles and Fuel Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the evaporative (EVAP) emission canister purge solenoid connector.
3. Disconnect the vacuum hoses from the EVAP canister purge solenoid.
4. Unclip the EVAP emission canister purge solenoid from the mounting bracket.

### Installation Procedure

1. Clip the EVAP emission canister purge solenoid to the mounting bracket.
2. Install the vacuum hoses to the EVAP canister purge solenoid.
3. Install the EVAP emission canister purge solenoid connector.
4. Connect the negative battery cable.