Hood Hinge Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Hood Hold-Open Device Caution in the Preface section.

1. Remove the hood. Refer to Hood Replacement .
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
3. Remove the bolts on the top of the fender.
4. Remove the hood hinge bolts (1).
5. Remove the hood hinge (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the hood hinge (2) with the bolts (1).

Tighten
Tighten the hood to hinge bolts to 25 N·m (18 lb ft).

2. Install the bolts along the top of the fender.

Tighten
Tighten the upper fender bolts to 10 N·m (89 lb in).

3. Install the air inlet grille. Refer to Air Inlet Grille Panel Replacement .
4. Install the hood. Refer to Hood Replacement .